BUILD PHYSICS  |  GUIDED INVESTIGATION
ATWOOD MACHINE
Mass difference, total mass, tension, and acceleration
	Name: ____________________________
	Period: ____________
	Date: ______________



	INVESTIGATION QUESTION  How do mass difference and total mass determine the acceleration of an Atwood machine?


	TIME
30 minutes
	SIMULATION
BuildPhysics > Atwood machine
	UNIT 2
Force & Translational Dynamics


Learning targets
• Apply Newton's second law to a two-mass system.
• Test acceleration while total mass or mass difference is controlled.
• Compare rope tension with the weights of the two masses.
Model before you measure
	The pulley is massless in this preset. Label the heavier side m₁ and choose its downward direction as positive.
	a = (m1 − m2)g/(m1 + m2)


	Important: Use g = 9.8 m/s². Keep both masses clear of the pulley and floor, and reset before each run.


Pre-lab prediction | 4 minutes
1. What happens when the two masses are equal?
__________________________________________________________________________________________
2. If total mass stays constant, how should acceleration change as the mass difference grows?
__________________________________________________________________________________________
3. If mass difference stays constant but total mass increases, how should acceleration change?
__________________________________________________________________________________________


	PART A  Keep total mass constant


Setup | 3 minutes
□ Load Atwood machine. Confirm the pulley is massless and the rope is connected to both masses.
□ Set m₁ and m₂ so their total is 3.0 kg for every Part A trial.
□ Select a mass to read acceleration and select the rope or mass to read tension.
□ Reset, run briefly, pause before either mass reaches an obstacle, and record.
	Control: Keep m₁ + m₂ = 3.0 kg. The independent variable is the mass difference m₁ − m₂.


Data table | 10 minutes
	m₁
(kg)
	m₂
(kg)
	m₁ − m₂
(kg)
	Predicted a
(m/s²)
	Measured a
(m/s²)

	1.50
	1.50
	
	
	

	1.75
	1.25
	
	
	

	2.00
	1.00
	
	
	

	2.25
	0.75
	
	
	

	2.50
	0.50
	
	
	


[image: ]
4. Plot measured acceleration versus mass difference. Draw a best-fit line.


	PART B  Keep mass difference constant


Total-mass test | 6 minutes
	Control: Keep m₁ − m₂ = 1.0 kg while increasing both masses.


	m₁
(kg)
	m₂
(kg)
	Predicted a
(m/s²)
	Measured a
(m/s²)

	2.0
	1.0
	
	

	3.0
	2.0
	
	

	4.0
	3.0
	
	


Analysis | 8 minutes
5. What did the slope in Part A represent when total mass was 3.0 kg?
_______________________________________________________________________________________________
6. Why did equal masses produce zero acceleration even though both weights were nonzero?
_______________________________________________________________________________________________
7. Why did acceleration decrease in Part B while the mass difference stayed 1.0 kg?
_______________________________________________________________________________________________
8. For the 2.0 kg and 1.0 kg trial, calculate the predicted rope tension using either mass.
_______________________________________________________________________________________________
Claim-Evidence-Reasoning conclusion
	Evaluate this statement: “Only the difference between the two masses determines an Atwood machine's acceleration.”


	CLAIM
	Accept, reject, or revise the statement.



	EVIDENCE
	Cite at least two measurements or graph features.



	REASONING
	Connect your evidence to the force model and Newton's laws.




Exit ticket
Predict the acceleration of an ideal Atwood machine with masses 3.0 kg and 1.0 kg. Use g = 9.8 m/s².
____________________________________________________________________________________________
____________________________________________________________________________________________
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